SKIP CONNECTION

The second proposal is to use a skip-connection from input to the reconstruction layer. In SR, a low-resolution image (input) and a high-resolution image (output) share the same information to a large extent. Exact copy of input, however, is likely to be attenuated during many forward passes. We explicitly connect the input to the layers for output reconstruction. This is particularly effective when input and output are highly correlated.















